mkvmerge -- Об’єднує мультимедійні потоки в файли Matroska

mkvmerge -- Об’єднує мультимедійні потоки в файли Matroska(tm)

# 1. Короткий опис

mkvmerge global options {-o out} options1 {file1} options2 {file2} @options-file.json

# 2. Опис

Ця програма бере вхідні дані з кількох медіа-файлів і об’єднує їхні потоки (усі або лише виділені) в файл Matroska(tm); див. веб-сайт Matroska.

Important:

Важливим є порядок параметрів командного рядка. Будь ласка, прочитайте розділ "Порядок опцій", якщо ви новачок у програмі.

## 2.1. Загальні опції

Option | Description
--- | ---
-v, --verbose | Підвищіти багатослівність
-q, --quiet | Пригнітити вихід статусу.
-o, --output file-name | Записує у файл file-name. Якщо використовується розщеплення, цей параметр розглядається дещо інакше. Додаткову інформацію див. у поясненнях про параметр --split.

-w, --webm

Створює файл, сумісний із WebM. Це також увімкнено, якщо вихідний файл має розширення "webm". Цей режим передбачає кілька обмежень. Єдиними дозволеними кодеками є відео VP8, VP9 та аудіо Opus, Vorbis. Елемент заголовка DocType змінюється на "webm".

Для глав і тегів дозволяється лише підмножина елементів. mkvmerge(1) автоматично видалить усі елементи, не дозволені специфікацією.

--title title | Встановлює загальну назву вихідного файлу, напр. назва фільму.
--default-language language-code | Встановлює код мови за замовчуванням, який використовуватиметься для треків, для яких не встановлено мову за допомогою параметра --language, а також для якого вихідний контейнер не надає мову. Код мови за замовчуванням — 'und' для 'невизначено'.

## 2.2. Обробка інформації про сегменти (загальні параметри)

Option | Description
--- | ---
--segmentinfo filename.xml | Прочитати інформацію про сегменти з файлу XML. Цей файл може містити сімейство сегментів UID, сегмент UID, елементи попереднього та наступного сегментів UID. Приклад файлу та DTD включені в дистрибутив MKVToolNix. Додаткову інформацію див. у розділі "файли XML із інформацією про сегмент".

--segment-uid SID1,SID2,...

Встановлює UID сегмента для використання. Це розділений комами список 128-бітних сегментних UID у звичайній формі UID: шістнадцяткові числа з або без "0x" префікс із пробілами чи без, точно 32 розряди».

Якщо SID починається з "=", то його залишок інтерпретується як ім’я файлу Matroska, UID сегмента якого читається та використовується.

Кожен створений файл містить один сегмент, і кожен сегмент має один UID сегмента. Якщо вказано більше UID сегментів, ніж створено сегментів, то зайві UID ігноруються. Якщо вказано менше UID, ніж створено сегментів, для них будуть створені випадкові UID.

## 2.3. Обробка глав і тегів (загальні параметри)

Option | Description
--- | ---

--chapter-language language-code

Встановлює код мови ISO 639-2, який записується для кожного запису глави. За замовчуванням 'eng'. Перегляньте розділ про "глави" нижче, щоб дізнатися більше.

Цей параметр можна використовувати як для простих файлів глав, так і для вихідних файлів, які містять глави, але не містять інформації про мову глав, наприклад файли MP4 і OGM.

Мова, встановлена цією опцією, також використовується, коли глави створюються за допомогою параметра --generate-chapters.

--chapter-charset character-set | Встановлює набір символів, який використовується для перетворення в UTF-8 для простих файлів глав. Перегляньте розділ про текстові файли та набори символів, щоб дізнатися, як mkvmerge(1) перетворює між наборами символів. Цей перемикач також застосовується до глав, які скопійовані з певних типів контейнерів, наприклад файли Ogg/OGM і MP4. Додаткову інформацію див. у розділі про глави нижче.

--chapter-sync d[,o[/p]]

Налаштуйте мітки часу глав у наступному вихідному файлі на d мс. Крім того, ви можете використовувати параметр --sync зі спеціальним ідентифікатором доріжки -2 (див. розділ спеціальні ID доріжок).

o/p: налаштуйте мітки часу на o/p, щоб виправити лінійні зсуви. Параметр p за замовчуванням має значення 1, якщо його опустити. І o, і p можуть бути числами з плаваючою комою.

Значення за замовчуванням: немає ручної корекції синхронізації (це те саме, що d = 0 і o/p = 1.0).

Цю опцію можна використовувати кілька разів, щоб вхідний файл застосовувався до кількох доріжок, вибираючи щоразу різні ідентифікатори доріжок.

--generate-chapters mode

mkvmerge(1) може створювати глави автоматично. На даний момент підтримуються наступні два режими:

- 'when-appending' – цей режим створює одну главу на початку і одну главу щоразу, коли додається файл.

  Цей режим також працює з режимами розділення 'parts:' і 'parts-frames:'. Для цих режимів буде створено одну главу для кожного доданого діапазону міток часу (тих, чиї початкові мітки часу мають префікс '+').

  Note:

  mkvmerge(1) вимагає наявності відео або аудіо доріжки, щоб можна було визначити, коли буде додано новий файл. Якщо одна або кілька відео доріжок мультиплексовані, використовується перша з них. В іншому випадку використовується перша звукова доріжка.

- 'interval: time-spec' – цей режим створює одну главу з фіксованими інтервалами, заданими time-spec. Формат у формі HH:MM:SS.nnnnnnnnn або число, за яким слідує одна з одиниць 's', 'ms' або 'us'.

  Приклад: --generate-chapters interval:45s

Назви нових глав керуються опцією --generate-chapters-name-template. Мова встановлюється за допомогою --chapter-language, яка має бути наведена перед --generate-chapters.

--generate-chapters-name-template template

Це встановлює шаблон назви для імен глав, створених за допомогою опції --generate-chapters. Якщо ця опція не використовується, буде використано стандартне значення «Глава <NUM:2>».

Існує кілька змінних, які можна використовувати в шаблоні, що замінюються їхніми фактичними значеннями під час створення глави. Рядок '<NUM>' буде замінено номером глави. Рядок '<START>' буде замінено міткою часу початку глави.

Рядки '<FILE_NAME>' і '<FILE_NAME_WITH_EXT>' заповнюються лише під час створення глав для доданих файлів. Вони будуть замінені іменем доданого файлу без його розширення. Зауважте, що вставляються лише базове ім’я та розширення файлу, а не каталог чи диск.

Ви можете вказати мінімальну кількість місць для номера глави за допомогою '<NUM:places>', наприклад '<NUM:3>'. Отримане число буде доповнено провідними нулями, якщо кількість місць менше зазначеної.

Ви можете керувати форматом, який використовується початковою міткою часу, за допомогою <START:format>. Формат за замовчуванням має значення '%H:%M:%S', якщо жодного не вказано. Допустимі коди формату:

- %h – години

- %H – години, два розряди доповнені провідними нулями

- %m – хвилини

- %M – хвилини, два розряди доповнені провідними нулями

- %s – секунди

- %S – секунди, два розряди доповнені провідними нулями

- %n – наносекунди, дев'ять розрядів доповнені провідними нулями

- %<1-9>n – наносекунди дев'ять розрядів доповнені провідними нулями (напр. три розряди з %3n)

--cue-chapter-name-format format

mkvmerge(1) підтримує читання списків CUE для аудіофайлів як вхідних даних для глав. Списки CUE зазвичай містять записи PERFORMER і TITLE для кожного запису індексу. mkvmerge(1) використовує ці два рядки для створення назви глави. За допомогою цієї опції можна встановити формат, який використовується для цього імені.

Якщо цей параметр не вказано, mkvmerge(1) за замовчуванням має формат '%p - %t' (виконавець, за яким слідує пробіл, тире, інший пробіл і заголовок).

Якщо вказано формат, то все, крім наступних метасимволів, копіюється як є, а метасимволи замінюються таким чином:

- %p замінюється на рядок PERFORMER поточного запису,

- %t замінюється на рядок TITLE поточного запису,

- %n замінюється на номер поточної доріжки та

- %N замінюється номером поточної доріжки, доповненою початковим нулем, якщо це < 10.

--chapters file-name | Прочитайте інформацію про главу із файлу file-name. Перегляньте розділ про глави нижче, щоб дізнатися більше.
--global-tags file-name | Читає глобальні теги з файлу file-name. Додаткову інформацію див. у розділі про теги нижче.

## 2.4. Загальне керування виводом (розширені глобальні параметри)

Option | Description
--- | ---
--track-order FID1:TID1,FID2:TID2,... | Цей параметр змінює порядок, у якому створюються доріжки для вхідного файлу. Аргументом є список ID пар, розділених комами. Кожна пара містить спочатку ID файлу (FID1), який є просто номером файлу в командному рядку, починаючи з 0 і потім ID доріжки (TID1) із цього файла. Якщо деякі ID доріжок пропущені, ці доріжки створюються після того, як були створені доріжки, задані цією опцією.

--cluster-length spec

Обмежте кількість блоків даних або тривалість даних у кожному кластері. Параметр spec може бути числом n без одиниць або числом d з постфіксом 'ms'.

Якщо одиниця не використовується, mkvmerge(1) помістить щонайбільше n блоків даних у кожному кластері. Максимальна кількість блоків – 65535.

Якщо число d має постфікс 'ms', тоді mkvmerge(1) розміщує щонайбільше d мілісекунд даних у кожен кластер. Діапазон для d — від '100 мс' до '32000 мс'.

mkvmerge(1) за замовчуванням містить щонайбільше 65535 блоків даних і 5000 мс даних у кластер.

Програми, які намагаються знайти певний фрейм, можуть шукати лише безпосередньо кластер, а потім читати весь кластер. Тому створення більших кластерів може призвести до неточного або повільного пошуку.

--clusters-in-meta-seek | Повідомляє mkvmerge(1) створити мета-елемент пошуку в кінці файлу, що містить усі кластери. Дивіться також розділ про макет файлу Matroska.

--timestamp-scale factor

Примусово встановлює коефіцієнт масштабу мітки часу в factor. Припустимі значення знаходяться в діапазоні 1000..10000000 або спеціальному значенні -1.

Зазвичай mkvmerge(1) використовує значення 1000000, що означає, що мітки часу та тривалість мають точність 1 мс. Для файлів, які не містять відео доріжку, але мають принаймні одну звукову mkvmerge(1) автоматично вибере коефіцієнт масштабу мітки часу, щоб усі мітки часу та тривалість мали точність до одного звукового зразка. Це спричиняє більші накладні витрати, але забезпечує точний пошук і витягування.

Якщо використовується спеціальне значення -1, то mkvmerge(1) використовує точність зразка, навіть якщо є відеодоріжка.

--enable-durations | Записує тривалість для всіх блоків. Це збільшить розмір файлу і на даний момент не пропонує жодної додаткової цінності для програвачів.
--no-cues | Повідомляє mkvmerge(1) не створювати та записувати дані cue, які можна порівняти з індексом у AVI. Файли Matroska(tm) можна відтворювати без даних cue, але пошук, ймовірно, буде неточним і повільнішим. Використовуйте це, лише якщо ви справді відчайдушно потребуєте місця або для тестування. Дивіться також параметр --cues, який можна вказати для кожного вхідного файлу.
--no-date | За замовчуванням mkvmerge(1) встановлює в інформаційному полі сегмента "дата" час і дату початку мультиплексування. За допомогою цієї опції це поле взагалі не записується.
--disable-lacing | Відключає лейсінг для всіх доріжок. Це збільшить розмір файлу, особливо якщо в ньому багато звукових доріжок. Цей варіант не призначений для повсякденного використання.
--disable-track-statistics-tags | Зазвичай mkvmerge(1) записує певні теги зі статистикою для кожної доріжки. Якщо такі теги вже є, вони будуть перезаписані. Теги: BPS, DURATION, NUMBER_OF_BYTES і NUMBER_OF_FRAMES. Увімкнення цієї опції запобігає mkvmerge(1) від записування цих тегів і від дотику до будь-яких існуючих тегів з однаковими іменами.
--disable-language-ietf | Зазвичай mkvmerge(1) записує нові мовні елементи IETF BCP 47 на додаток до спадкових мовних елементів у заголовках, главах та тегах доріжок. Якщо використовується ця опція, записуються лише спадкові елементи.

## 2.5. Розділення файлів, зв’язування, додавання та конкатенація (більш глобальні параметри)

Option | Description
--- | ---

--split specification

Розділяє вихідний файл після заданого розміру або часу. Зверніть увагу, що доріжки можна розділити лише перед ключовим кадром. Тому точка розділення може трохи відрізнятися від того, що вказав користувач.

На даний момент mkvmerge(1) підтримує такі режими:

1. Розділення за розміром.

   Синтаксис: --split [size:]d[k|m|g]

   Приклад: --split size:700m or --split 150000000

   Параметр d може закінчуватися на 'k', 'm' або 'g', щоб вказати, що розмір у КБ, МБ або ГБ відповідно. В іншому випадку передбачається розмір у байтах. Після того як поточний вихідний файл досягне цього обмеження розміру, буде запущено новий.

   Префікс 'size:' може бути опущений з міркувань сумісності.

2. Розділення за тривалістю.

   Синтаксис: --split [duration:]HH:MM:SS.nnnnnnnnn|ds

   Приклад: --split duration:00:60:00.000 or --split 3600s

   Параметр повинен мати форму HH:MM:SS.nnnnnnnn для визначення тривалості з точністю до наносекунди або бути числом d, за яким слідує літера 's' для тривалості в секундах. Параметр HH – це кількість годин, MM - хвилин, SS - секунд і nnnnnnnn - наносекунд. Як кількість годин, так і кількість наносекунд можна опустити. Після коми може бути до дев’яти цифр. Після того, як тривалість вмісту поточного виводу досягне цієї межі, буде запущено новий вихідний файл.

   Префікс 'duration:' може бути опущено з міркувань сумісності.

3. Розділення за мітками часу.

   Синтаксис: --split timestamps: A[,B[,C...]]

   Приклад: --split timestamps:00:45:00.000,01:20:00.250,6300s

   Параметри A, B, C тощо повинні мати той самий формат, що й ті, що використовуються для тривалості (див. вище). Список міток часу розділяється комами. Після того, як вхідний потік досяг мітки часу поточної точки розділення, створюється новий файл. Тоді використовується наступна точка розділення, зазначена в цьому списку.

   Не можна опускати префікс 'timestamps:'.

4. Зберігання певних частин шляхом вказівки діапазонів міток часу, відкидаючи інші.

   Синтаксис: --split parts: start1-end1[,[+]start2-end2[,[+]start3-end3...]]

   Приклади:

   1. --split parts:00:01:20-00:02:45,00:05:50-00:10:30

   2. --split parts:00:01:20-00:02:45,+00:05:50-00:10:30

   3. --split parts:-00:02:45,00:05:50-

   Режим parts повідомляє mkvmerge(1) зберігати певні діапазони міток часу, відкидаючи інші. Діапазони, які потрібно зберегти, мають бути перелічені після ключового слова parts: і розділені комами. Сам діапазон складається з мітки часу початку та кінця у форматі однакового вигляду, який приймаєтся в різних варіантах --split (наприклад, 00:01:20 і 80s посилаються на ту саму мітку часу).

   Якщо мітка часу початку не вказана, то за замовчуванням буде використана мітка часу кінця попереднього діапазону. Якщо попереднього діапазону не було, то за замовчуванням це початок файлу (див. приклад 3).

   Якщо мітка часу завершення не вказана, за замовчуванням буде використан кінець вихідних файлів, що в основному повідомляє mkvmerge(1) залишити решту (див. приклад 3).

   Зазвичай кожен діапазон записується в новий файл. Це можна змінити, щоб послідовні діапазони записувалися в один файл. Для цього користувач повинен поставити перед міткою часу початку символ +. Це повідомляє mkvmerge(1) не створювати новий файл, а замість цього додати діапазон до того самого файлу, в який був записаний попередній діапазон. Мітки часу будуть налаштовані таким чином, щоб у вихідному файлі не було пробілів, навіть якщо у вхідному файлі був пробіл у двох діапазонах.

   У прикладі 1 mkvmerge(1) створить два файли. Перший міститиме вміст, починаючи з 00:01:20 до 00:02:45. Другий файл міститиме вміст, починаючи з 00:05:50 до 00:10:30.

   У прикладі 2 mkvmerge(1) створить лише один файл. Цей файл міститиме як вміст, починаючи з 00:01:20 до 00:02:45, так і вміст, починаючи з 00:05:50 до 00:10:30.

   У прикладі 3 mkvmerge(1) створить два файли. Перший міститиме вміст від початку вихідних файлів до 00:02:45. Другий файл міститиме вміст, починаючи з 00:05:50 до кінця вихідних файлів.

   Note:

   Зверніть увагу, що mkvmerge(1) виконує розділення лише по позиціях ключових кадрів. Це стосується як початку, так і кінця кожного діапазону. Тому, навіть якщо мітка часу завершення знаходиться між двома ключовими кадрами mkvmerge(1) продовжить виведення кадрів до наступного ключового кадру, але не включаючи його.

5. Зберігання певних частин шляхом вказування діапазонів номерів кадрів/полів, відкидаючи інше.

   Синтаксис: --split parts-frames: start1-end1[,[+]start2-end2[,[+]start3-end3...]]

   Приклади:

   1. --split parts-frames:137-258,548-1211

   2. --split parts-frames:733-912,+1592-2730

   3. --split parts-frames:-430,2512-

   Режим parts-frames повідомляє mkvmerge(1) зберегти певні діапазони номерів кадрів/полів, відкидаючи інше. Діапазони, які потрібно зберегти, мають бути перелічені після ключового слова parts-frames: і розділені комами. Сам діапазон складається з початкового та кінцевого номера кадра/поля. Нумерація починається з 1.

   Якщо початковий номер не вказано, то за замовчуванням буде використовуватися кінцевий номер попереднього діапазону. Якщо попереднього діапазону не було, то за замовчуванням це буде початок файлу (див. приклад 3).

   Якщо кінцевий номер не вказано, то за замовчуванням ним буде кінець вихідних файлів, що в основному повідомляє mkvmerge(1) залишити решту (див. приклад 3).

   Зазвичай кожен діапазон записується в новий файл. Це можна змінити, щоб послідовні діапазони записувалися в один файл. Для цього користувач повинен поставити перед початковим номером знак +. Це повідомляє mkvmerge(1) не створювати новий файл, а замість цього додати діапазон до того самого файлу, в який був записаний попередній діапазон. Мітки часу будуть налаштовані таким чином, щоб у вихідному файлі не було пробілів, навіть якщо у вхідному файлі був пробіл у двох діапазонах.

   Note:

   Зверніть увагу, що mkvmerge(1) виконує розділення лише по позиціях ключових кадрів. Це стосується як початку, так і кінця кожного діапазону. Тому, навіть якщо кінцевий кадр/номер поля знаходиться між двома ключовими кадрами mkvmerge(1) продовжить виведення кадрів до наступного ключового кадру, але без урахування його.

   У прикладі 1 mkvmerge(1) створить два файли. Перший міститиме вміст, починаючи з першого ключового кадру 137 до 258. Другий файл міститиме вміст від 548 до 1211.

   У прикладі 2 mkvmerge(1) створить лише один файл. Цей файл міститиме вміст, починаючи з 733 до 912, і вміст, починаючи з 1592 до 2730.

   У прикладі 3 mkvmerge(1) створить два файли. Перший міститиме вміст від початку вихідних файлів до 430. Другий файл міститиме вміст, починаючи з 2512 до кінця вихідних файлів.

   У цьому режимі розглядається лише перша відеодоріжка, яка виводиться. Якщо відеодоріжка не виводиться, розділення не відбудеться.

   Note:

   Числа, дані з цим аргументом, інтерпретуються на основі числа блоків Matroska(tm), що виводяться. Єдиний блок Matroska(tm) містить або повний кадр (для прогресивного вмісту) або одне поле (для вмісту з чередуванням). mkvmerge не розрізняє їх і просто підраховує кількість блоків. Наприклад: якщо ви хочете розділити після 25-го повного кадру з вмістом чередування, вам доведеться в якості точки поділу вказати 50 (два поля на повний кадр).

6. Розділення на певні кадри/поля.

   Синтаксис: --split frames: A[,B[,C...]]

   Приклад: --split frames:120,237,891

   Усі параметри A, B, C тощо мають бути цілими додатними числами. Нумерація починається з 1. Список номерів кадрів/полів розділяється комами. Після того, як вхідний потік досягнув номера кадру/поля поточної точки розділення, створюється новий файл. Тоді використовується наступна точка розділення, зазначена в цьому списку.

   Не можна опускати префікс 'frames:'.

   У цьому режимі розглядається лише перша відеодоріжка, яка виводиться. Якщо відеодоріжка не виводиться, розділення не відбудеться.

   Note:

   Числа, дані з цим аргументом, інтерпретуються на основі числа блоків Matroska(tm), що виводяться. Єдиний блок Matroska(tm) містить або повний кадр (для прогресивного вмісту) або одне поле (для вмісту з чередуванням). mkvmerge не розрізняє їх і просто підраховує кількість блоків. Наприклад: якщо ви хочете розділити після 25-го повного кадру з вмістом чередування, вам доведеться в якості точки поділу вказати 50 (два поля на повний кадр).

7. Розділення перед конкретними главами.

   Синтаксис: --split chapters:all or --split chapters: A[,B[,C...]]

   Приклад: --split chapters:5,8

   Усі параметри A, B, C тощо мають бути цілими додатними числами. Нумерація починається з 1. Список номерів глав розділяється комами. Розділення відбудеться безпосередньо перед першим ключовим кадром, мітка часу якого дорівнює або більша за початкову мітку часу для глав, номери яких вказані. Глава, що починається з 0s, ніколи не розглядається для розділення та відкидається без змін.

   Ключове слово all можна використовувати замість того, щоб перераховувати всі номери глав вручну.

   Не можна опускати префікс 'chapters:'

   Note:

   Формат файлу Matroska(tm) підтримує довільні глибоко вкладені структури глав, які називаються «записами видання» та «атомами глав». Однак цей режим враховує лише найвищий рівень глав у всіх записах видання.

Для цього режиму розділення ім’я вихідного файлу обробляється інакше, ніж для звичайної операцій. Він може містити printf, наприклад, вираз '%d', включаючи необов'язкову ширину поля, напр. '%02d'. Якщо це так, то номер поточного файлу буде відформатовано відповідним чином і вставлено в цю точку імені файлу. Якщо такого шаблону немає, то перед розширенням файлу передбачається шаблон '-%03d': '-o output.mkv' призведе до 'output-001.mkv' тощо. Якщо розширення немає, до імені буде додано '-%03d'.

Іншим можливим шаблоном є '%c', який буде замінено назвою першої глави у файлі. Зауважте, що коли присутній '%c', шаблон '-%03d' не буде додано автоматично.

--link | Зв’язує файли один з одним під час розділення вихідного файлу. Додаткову інформацію див. у розділі з'язування файлів нижче
--link-to-previous segment-UID | Зв’язує перший вихідний файл із сегментом із UID сегмента, заданим параметром segment-UID. Додаткову інформацію див. у розділі з'язування файлів нижче. Якщо SID починається з "=", то його залишок інтерпретується як ім’я файлу Matroska, UID сегмента якого читається та використовується.
--link-to-next segment-UID | Зв’язує останній вихідний файл із сегментом із UID сегмента, заданим параметром segment-UID. Додаткову інформацію див. у розділі з'язування файлів нижче. Якщо SID починається з "=", то його залишок інтерпретується як ім’я файлу Matroska, UID сегмента якого читається та використовується.

--append-mode mode

Визначає, як обчислюються мітки часу під час додавання файлів. Параметр mode може мати два значення: 'file' (за замовчуванням) і 'track'.

Коли mkvmerge додає доріжку (відтепер називається 'track2_1') з другого файлу (що зветься 'file2') до доріжки (що зветься 'track1_1') з першого файлу (що зветься 'file1'), то він має зміщувати всі мітки часу для 'track2_1' на певну величину. Для режиму 'file' ця сума є найвищою міткою часу, що зустрічається в 'file1', навіть якщо ця мітка часу була з іншої доріжки, ніж 'track1_1'. У режимі доріжки зсув є найвищою міткою часу 'track1_1'.

На жаль, mkvmerge не може визначити, який режим надійно використовувати. Тому він за замовчуванням працює в режимі 'file'. Режим 'file' зазвичай краще працює для файлів, які були створені незалежно один від одного; напр. під час додавання файлів AVI або MP4. Режим 'track' може працювати краще для джерел, які по суті є лише частинами одного великого файлу, напр. для файлів VOB і EVO.

Доріжки субтитрів завжди розглядаються так, ніби режим 'file' був активним, навіть якщо режим 'track' насправді є.

--append-to SFID1:STID1:DFID1:DTID1[,...]

Цей параметр визначає, до якої доріжки буде додано іншу доріжку. Кожна специфікація містить чотири ID: ID файлу, ID треку, другий ID файлу та другий ID треку. Перша пара, "ID вихідного файлу" та "ID вихідної доріжки", визначає доріжку, яка має бути додана. Друга пара, "ID файлу призначення" та "ID доріжки призначення", визначає доріжку, до якої додається перша.

Якщо ця опція була пропущена, використовується стандартне зіставлення. Це стандартне зіставлення додає кожну доріжку з поточного файлу до доріжки з попереднього файлу з тим самим ID доріжки. Це дозволяє легко додавати, якщо фільм було розділено на дві частини і обидва файли мають однакову кількість доріжок та ID доріжок за допомогою команди mkvmerge -o output.mkv part1.mkv +part2.mkv.

+

Одиночний '+' викликає приєднання наступного файлу, а не його додавання. '+' також можна поставити перед наступним ім’ям файлу. Тому наступні дві команди є еквівалентними:

    $ mkvmerge -o full.mkv file1.mkv + file2.mkv
    $ mkvmerge -o full.mkv file1.mkv +file2.mkv

[ file1 file2 ]

Якщо кілька імен файлів містяться в парі квадратних дужок, то другий і всі наступні файли будуть додані до першого файлу, названого в дужках.

Це альтернативний синтаксис використання '+' між іменами файлів. Тому наступні дві команди є еквівалентними:

    $ mkvmerge -o full.mkv file1.mkv + file2.mkv
    $ mkvmerge -o full.mkv '[' file1.mkv file2.mkv ']'

=

For certain file types (MPEG program streams = VOBs) mkvmerge(1) normally looks for files in the same directory as an input file that have the same base name and only differ in their running number (e.g. 'VTS_01_1.VOB', 'VTS_01_2.VOB', 'VTS_01_3.VOB' etc) and treats all of those files as if they were concatenated into a single big file. This option, a single '=', causes mkvmerge not to look for those additional files.

The '=' can also be put in front of the next file name. Therefore the following two commands are equivalent:

    $ mkvmerge -o full.mkv = file1.mkv
    $ mkvmerge -o full.mkv =file1.mkv

( file1 file2 )

If multiple file names are contained in a pair of parenthesis then those files will be treated as if they were concatenated into a single big file consisting of the content of each of the files one after the other.

This can be used for e.g. VOB files coming from a DVD or MPEG transport streams. It cannot be used if each file contains its own set of headers which is usually the case with stand-alone files like AVI or MP4.

Putting a file name into parenthesis also prevents mkvmerge(1) from looking for additional files with the same base name as described in option =. Therefore these two command lines are equivalent:

    $ mkvmerge -o out.mkv = file.mkv
    $ mkvmerge -o out.mkv '(' file.mkv ')'

Several things should be noted:

1. There must be spaces both after the opening and before the closing parenthesis.

2. Every parameter between parenthesis is interpreted as a file name. Therefore all options applying to this logical file must be listed before the opening parenthesis.

3. Some shells treat parenthesis as special characters. Hence you must escape or quote them as shown in the example above.

## 2.6. Attachment support (more global options)

Option | Description
--- | ---
--attachment-description description | Plain text description of the following attachment. Applies to the next --attach-file or --attach-file-once option.
--attachment-mime-type MIME type | MIME type of the following attachment. Applies to the next --attach-file or --attach-file-once option. A list of officially recognized MIME types can be found e.g. at the IANA homepage. The MIME type is mandatory for an attachment.
--attachment-name name | Sets the name that will be stored in the output file for this attachment. If this option is not given then the name will be derived from the file name of the attachment as given with the --attach-file or the --attach-file-once option.

--attach-file file-name, --attach-file-once file-name

Creates a file attachment inside the Matroska(tm) file. The MIME type must have been set before this option can used. The difference between the two forms is that during splitting the files attached with --attach-file are attached to all output files while the ones attached with --attach-file-once are only attached to the first file created. If splitting is not used then both do the same.

mkvextract(1) can be used to extract attached files from a Matroska(tm) file.

## 2.7. Options that can be used for each input file

Option | Description
--- | ---

-a, --audio-tracks [!]n,m,...

Copy the audio tracks n, m etc. The numbers are track IDs which can be obtained with the --identify switch. They're not simply the track numbers (see section track IDs). Default: copy all audio tracks.

Instead of track IDs you can also provide ISO 639-2 language codes. This will only work for source files that provide language tags for their tracks.

Default: copy all tracks of this kind.

If the IDs are prefixed with ! then the meaning is reversed: copy all tracks of this kind but the ones listed after the !.

-d, --video-tracks [!]n,m,...

Copy the video tracks n, m etc. The numbers are track IDs which can be obtained with the --identify switch. They're not simply the track numbers (see section track IDs). Default: copy all video tracks.

Instead of track IDs you can also provide ISO 639-2 language codes. This will only work for source files that provide language tags for their tracks.

If the IDs are prefixed with ! then the meaning is reversed: copy all tracks of this kind but the ones listed after the !.

-s, --subtitle-tracks [!]n,m,...

Copy the subtitle tracks n, m etc. The numbers are track IDs which can be obtained with the --identify switch. They're not simply the track numbers (see section track IDs). Default: copy all subtitle tracks.

Instead of track IDs you can also provide ISO 639-2 language codes. This will only work for source files that provide language tags for their tracks.

If the IDs are prefixed with ! then the meaning is reversed: copy all tracks of this kind but the ones listed after the !.

-b, --button-tracks [!]n,m,...

Copy the button tracks n, m etc. The numbers are track IDs which can be obtained with the --identify switch. They're not simply the track numbers (see section track IDs). Default: copy all button tracks.

Instead of track IDs you can also provide ISO 639-2 language codes. This will only work for source files that provide language tags for their tracks.

If the IDs are prefixed with ! then the meaning is reversed: copy all tracks of this kind but the ones listed after the !.

--track-tags [!]n,m,... | Copy the tags for tracks n, m etc. The numbers are track IDs which can be obtained with the --identify switch (see section track IDs). They're not simply the track numbers. Default: copy tags for all tracks. If the IDs are prefixed with ! then the meaning is reversed: copy everything but the IDs listed after the !.

-m, --attachments [!]n[:all|first],m[:all|first],...

Copy the attachments with the IDs n, m etc to all or only the first output file. Each ID can be followed by either ':all' (which is the default if neither is entered) or ':first'. If splitting is active then those attachments whose IDs are specified with ':all' are copied to all of the resulting output files while the others are only copied into the first output file. If splitting is not active then both variants have the same effect.

The default is to copy all attachments to all output files.

If the IDs are prefixed with ! then the meaning is reversed: copy everything but the IDs listed after the !.

-A, --no-audio | Don't copy any audio track from this file.
-D, --no-video | Don't copy any video track from this file.
-S, --no-subtitles | Don't copy any subtitle track from this file.
-B, --no-buttons | Don't copy any button track from this file.
-T, --no-track-tags | Don't copy any track specific tags from this file.
--no-chapters | Don't copy chapters from this file.
-M, --no-attachments | Don't copy attachments from this file.
--no-global-tags | Don't copy global tags from this file.

-y, --sync TID:d[,o[/p]]

Adjust the timestamps of the track with the id TID by d ms. The track IDs are the same as the ones given with --identify (see section track IDs).

o/p: налаштуйте мітки часу на o/p, щоб виправити лінійні зсуви. Параметр p за замовчуванням має значення 1, якщо його опустити. І o, і p можуть бути числами з плаваючою комою.

Значення за замовчуванням: немає ручної корекції синхронізації (це те саме, що d = 0 і o/p = 1.0).

Цю опцію можна використовувати кілька разів, щоб вхідний файл застосовувався до кількох доріжок, вибираючи щоразу різні ідентифікатори доріжок.

--cues TID:none|iframes|all

Controls for which tracks cue (index) entries are created for the given track (see section track IDs). 'none' inhibits the creation of cue entries. For 'iframes' only blocks with no backward or forward references ( = I frames in video tracks) are put into the cue sheet. 'all' causes mkvmerge(1) to create cue entries for all blocks which will make the file very big.

The default is 'iframes' for video and subtitle tracks and 'none' for audio tracks. See also option --no-cues which inhibits the creation of cue entries regardless of the --cues options used.

Цю опцію можна використовувати кілька разів, щоб вхідний файл застосовувався до кількох доріжок, вибираючи щоразу різні ідентифікатори доріжок.

--default-track-flag TID[:bool]

Sets the "default track" flag for the given track (see section track IDs) if the optional argument bool is set to 1 or if it isn't present. The flag will be set if the source container doesn't provide that information and the user doesn't specify it via this option.

If the user does not explicitly select a track during playback, the player should select one of the tracks that has its "default track" flag set, taking user preferences such as their preferred language into account.

Цю опцію можна використовувати кілька разів, щоб вхідний файл застосовувався до кількох доріжок, вибираючи щоразу різні ідентифікатори доріжок.

--track-enabled-flag TID[:bool]

Sets the "track enabled" flag for the given track (see section track IDs) to the given value bool (0 or 1; defaults to 1 if not specified). Tracks are enabled by default if no option is specified for them and the source container doesn't provide this information either.

Only tracks whose "track enabled" flag is set should be considered for playback.

Цю опцію можна використовувати кілька разів, щоб вхідний файл застосовувався до кількох доріжок, вибираючи щоразу різні ідентифікатори доріжок.

--forced-display-flag TID[:bool] | Sets the "forced display" flag for the given track (see section track IDs) if the optional argument bool is set to 1 or if it isn't present. Use this for tracks containing onscreen text or foreign-language dialogue. Цю опцію можна використовувати кілька разів, щоб вхідний файл застосовувався до кількох доріжок, вибираючи щоразу різні ідентифікатори доріжок.
--forced-track TID[:bool] | Sets the "hearing impaired" flag for the given track (see section track IDs) if the optional argument bool is set to 1 or if it isn't present. This flag can be set if the track is suitable for users with hearing impairments. Цю опцію можна використовувати кілька разів, щоб вхідний файл застосовувався до кількох доріжок, вибираючи щоразу різні ідентифікатори доріжок.
--forced-track TID[:bool] | Sets the "visual impaired" flag for the given track (see section track IDs) if the optional argument bool is set to 1 or if it isn't present. This flag can be set if the track is suitable for users with visual impairments. Цю опцію можна використовувати кілька разів, щоб вхідний файл застосовувався до кількох доріжок, вибираючи щоразу різні ідентифікатори доріжок.

--default-track TID[:bool]

Sets the "text descriptions" flag for the given track (see section track IDs) if the optional argument bool is set to 1 or if it isn't present. This flag can be set if the track contains textual descriptions of video content suitable for playback via a text-to-speech system for a visually-impaired user.

Цю опцію можна використовувати кілька разів, щоб вхідний файл застосовувався до кількох доріжок, вибираючи щоразу різні ідентифікатори доріжок.

--forced-track TID[:bool] | Sets the "original language" flag for the given track (see section track IDs) if the optional argument bool is set to 1 or if it isn't present. This flag can be set if the track is in the content's original language (not a translation). Цю опцію можна використовувати кілька разів, щоб вхідний файл застосовувався до кількох доріжок, вибираючи щоразу різні ідентифікатори доріжок.
--forced-track TID[:bool] | Sets the "commentary" flag for the given track (see section track IDs) if the optional argument bool is set to 1 or if it isn't present. This flag can be set if the track contains commentary. Цю опцію можна використовувати кілька разів, щоб вхідний файл застосовувався до кількох доріжок, вибираючи щоразу різні ідентифікатори доріжок.
--blockadd TID:level | Keep only the BlockAdditions up to the level level for the given track. The default is to keep all levels. This option only affects certain kinds of codecs like WAVPACK4.
--track-name TID:name | Sets the track name for the given track (see section track IDs) to name.

--language TID:language

Sets the language for the given track (see section track IDs). Both ISO 639-2 language codes and ISO 639-1 country codes are allowed. The country codes will be converted to language codes automatically. All languages including their ISO 639-2 codes can be listed with the --list-languages option.

Цю опцію можна використовувати кілька разів, щоб вхідний файл застосовувався до кількох доріжок, вибираючи щоразу різні ідентифікатори доріжок.

-t, --tags TID:file-name | Read tags for the track with the number TID from the file file-name. See the section about tags below for details.
--aac-is-sbr TID[:0|1] | повідомляє If the source file is a Matroska(tm) file then the CodecID should be enough to detect SBR AAC. However, if the CodecID is wrong then this switch can be used to correct that. If mkvmerge wrongfully detects that an AAC file is SBR then you can add ':0' to the track ID.
--reduce-to-core TID | повідомляє Currently only DTS tracks are affected by this option. TrueHD tracks that contain an embedded AC-3 core are instead presented as two separate tracks for which the user can select which track to copy. For DTS such a scheme would not work as the HD extensions cannot be decoded by themselves – unlike the TrueHD data.
--remove-dialog-normalization-gain TID | повідомляє Currently only AC-3, DTS and TrueHD tracks are affected by this option.
--timestamps TID:file-name | Read the timestamps to be used for the specific track ID from file-name. These timestamps forcefully override the timestamps that mkvmerge(1) normally calculates. Read the section about external timestamp files.

--default-duration TID:x

Forces the default duration of a given track to the specified value. Also modifies the track's timestamps to match the default duration. The argument x must be postfixed with 's', 'ms', 'us', 'ns', 'fps', 'p' or 'i' to specify the default duration in seconds, milliseconds, microseconds, nanoseconds, 'frames per second', 'progressive frames per second' or 'interlaced frames per second' respectively. The number x itself can be a floating point number or a fraction.

If the default duration is not forced then mkvmerge will try to derive the track's default duration from the container and/or the encoded bitstream for certain track types, e.g. AVC/H.264 or MPEG-2.

This option can also be used to change the FPS of video tracks without having to use an external timestamp file.

--fix-bitstream-timing-information TID[:0|1]

Normally mkvmerge(1) does not change the timing information (frame/field rate) stored in the video bitstream. With this option that information is adjusted to match the container timing information. The container timing information can come from various sources: from the command line (see option --default-duration), the source container or derived from the bitstream.

Note:

This has only been implemented for AVC/H.264 video tracks so far.

--compression TID:n

Selects the compression method to be used for the track. Note that the player also has to support this method. Valid values are 'none', 'zlib' and 'mpeg4_p2'/'mpeg4p2'.

The compression method 'mpeg4_p2'/'mpeg4p2' is a special compression method called 'header removal' that is only available for MPEG4 part 2 video tracks.

The default for some subtitle types is 'zlib' compression. This compression method is also the one that most if not all playback applications support. Support for other compression methods other than 'none' is not assured.

## 2.8. Options that only apply to video tracks

Option | Description
--- | ---
-f, --fourcc TID:FourCC | Forces the FourCC to the specified value. Works only for video tracks in the 'MS compatibility mode'.
--display-dimensions TID:widthxheight | Matroska(tm) files contain two values that set the display properties that a player should scale the image on playback to: display width and display height. These values can be set with this option, e.g. '1:640x480'. Another way to specify the values is to use the --aspect-ratio or the --aspect-ratio-factor option (see below). These options are mutually exclusive.

--aspect-ratio TID:ratio|width/height

Matroska(tm) files contain two values that set the display properties that a player should scale the image on playback to: display width and display height. With this option mkvmerge(1) will automatically calculate the display width and display height based on the image's original width and height and the aspect ratio given with this option. The ratio can be given either as a floating point number ratio or as a fraction 'width/height', e.g. '16/9'.

Another way to specify the values is to use the --aspect-ratio-factor or --display-dimensions options (see above and below). These options are mutually exclusive.

--aspect-ratio-factor TID:factor|n/d | Another way to set the aspect ratio is to specify a factor. The original aspect ratio is first multiplied with this factor and used as the target aspect ratio afterwards. Another way to specify the values is to use the --aspect-ratio or --display-dimensions options (see above). These options are mutually exclusive.
--cropping TID:left,top,right,bottom | Sets the pixel cropping parameters of a video track to the given values.
--colour-matrix TID:n | Sets the matrix coefficients of the video used to derive luma and chroma values from red, green and blue color primaries. The parameter n is an integer rangeing from 0 and 10. Valid values and their meaning are: 0: GBR, 1: BT709, 2: unspecified, 3: reserved, 4: FCC, 5: BT470BG, 6: SMPTE 170M, 7: SMPTE 240M, 8: YCOCG, 9: BT2020 non-constant luminance, 10: BT2020 constant luminance
--colour-bits-per-channel TID:n | Sets the number of coded bits for a colour channel. A value of 0 indicates that the number of bits is unspecified.
--chroma-subsample TID:hori,vert | The amount of pixels to remove in the Cr and Cb channels for every pixel not removed horizontally/vertically. Example: For video with 4:2:0 chroma subsampling, the parameter should be set to TID:1,1.
--cb-subsample TID:hori,vert | The amount of pixels to remove in the Cb channel for every pixel not removed horizontally/vertically. This is additive with --chroma-subsample. Example: For video with 4:2:1 chroma subsampling, the parameter --chroma-subsample should be set to TID:1,0 and Cb-subsample should be set to TID:1,0.
--chroma-siting TID:hori,vert | Sets how chroma is sited horizontally/vertically (0: unspecified, 1: top collocated, 2: half).
--colour-range TID:n | Sets the clipping of the color ranges (0: unspecified, 1: broadcast range, 2: full range (no clipping), 3: defined by MatrixCoefficients/TransferCharacteristics).
--colour-transfer-characteristics TID:n | The transfer characteristics of the video. Valid values and their meaning are: 0: reserved, 1: ITU-R BT.709, 2: unspecified, 3: reserved, 4: gamma 2.2 curve, 5: gamma 2.8 curve, 6: SMPTE 170M, 7: SMPTE 240M, 8: linear, 9: log, 10: log sqrt, 11: IEC 61966-2-4, 12: ITU-R BT.1361 extended colour gamut, 13: IEC 61966-2-1, 14: ITU-R BT.2020 10 bit, 15: ITU-R BT.2020 12 bit, 16: SMPTE ST 2084, 17: SMPTE ST 428-1; 18: ARIB STD-B67 (HLG)
--colour-primaries TID:n | Sets the colour primaries of the video. Valid values and their meaning are: 0: reserved, 1: ITU-R BT.709, 2: unspecified, 3: reserved, 4: ITU-R BT.470M, 5: ITU-R BT.470BG, 6: SMPTE 170M, 7: SMPTE 240M, 8: FILM, 9: ITU-R BT.2020, 10: SMPTE ST 428-1, 22: JEDEC P22 phosphors
--max-content-light TID:n | Sets the maximum brightness of a single pixel (Maximum Content Light Level) in candelas per square meter (cd/m²). The value of n should be a non-negtive integer.
--max-frame-light TID:n | Sets the maximum brightness of a single full frame (Maximum Frame-Average Light Level) in candelas per square meter (cd/m²). The value of n should be a non-negtive integer.
--chromaticity-coordinates TID:red-x,red-y,green-x,green-y,blue-x,blue-y | Sets the red/green/blue chromaticity coordinates as defined by CIE 1931.
--white-colour-coordinates TID:x,y | Sets the white colour chromaticity coordinates as defined by CIE 1931.
--max-luminance TID:float | Sets the maximum luminance in candelas per square meter (cd/m²). The value should be less than 9999.99.
--min-luminance TID:float | Sets the minimum luminance in candelas per square meter (cd/m²). The value should be less than 999.9999.
--projection-type TID:method | Sets the video projection method used. Valid values are 0 (rectangular projection), 1 (equirectangular projection), 2 (cubemap projection) and 3 (mesh projection).
--projection-private TID:data | Sets private data that only applies to a specific projection. Data must be given as hex numbers with or without the "0x" prefix, with or without spaces.
--projection-pose-yaw TID:float | Specifies a yaw rotation to the projection.
--projection-pose-pitch TID:float | Specifies a pitch rotation to the projection.
--projection-pose-roll TID:float | Specifies a roll rotation to the projection.
--field-order TID:n | Sets the field order for the video track with the track ID TID. The order must be one of the following numbers: 0: progressive; 1: interlaced with top field displayed first and top field stored first; 2: undetermined field order; 6: interlaced with bottom field displayed first and bottom field stored first; 9: interlaced with bottom field displayed first and top field stored first; 14: interlaced with top field displayed first and bottom field stored first
--stereo-mode TID:n|keyword | Sets the stereo mode for the video track with the track ID TID. The mode can either be a number n between 0 and 14 or one of these keywords: 'mono', 'side_by_side_left_first', 'top_bottom_right_first', 'top_bottom_left_first', 'checkerboard_right_first', 'checkerboard_left_first', 'row_interleaved_right_first', 'row_interleaved_left_first', 'column_interleaved_right_first', 'column_interleaved_left_first', 'anaglyph_cyan_red', 'side_by_side_right_first', 'anaglyph_green_magenta', 'both_eyes_laced_left_first', 'both_eyes_laced_right_first'.

## 2.9. Options that only apply to text subtitle tracks

Option | Description
--- | ---

--sub-charset TID:character-set

Sets the character set for the conversion to UTF-8 for UTF-8 subtitles for the given track ID. If not specified the charset will be derived from the current locale settings. Note that a charset is not needed for subtitles read from Matroska(tm) files or from Kate streams, as these are always stored in UTF-8. See the section about text files and character sets for an explanation how mkvmerge(1) converts between character sets.

Цю опцію можна використовувати кілька разів, щоб вхідний файл застосовувався до кількох доріжок, вибираючи щоразу різні ідентифікатори доріжок.

## 2.10. Інші налаштування

Option | Description
--- | ---
-i, --identify file-name | Will let mkvmerge(1) probe the single file and report its type, the tracks contained in the file and their track IDs. If this option is used then the only other option allowed is the filename. The output format used for the result can be changed with the option --identification-format.
-J file-name | This is a convenient alias for "--identification-format json --identify file-name".

-F, --identification-format format

Determines the output format used by the --identify option. The following formats are supported: text (the default if this option isn't used) and json.

1. The text format is short and human-readable. It consists of one line per item found (container, tracks, attachments etc.).

   This format is not meant to be parsed. The output will be translated into the language mkvmerge(1) uses (see also --ui-language).

2. The json format outputs a machine-readable JSON representation. This format follows the JSON schema described in the following file:

   mkvmerge-identification-output-schema-v14.json

   All versions of the JSON schema are available both online and in the released source code archives.

--probe-range-percentage percentage | File types such as MPEG program and transport streams (.vob, .m2ts) require parsing a certain amount of data in order to detect all tracks contained in the file. This amount is 0.3% of the source file's size or 10 MB, whichever is higher. If tracks are known to be present but not found then the percentage to probe can be changed with this option. The minimum of 10 MB is built-in and cannot be changed.
-l, --list-types | Lists supported input file types.
--list-languages | Lists all languages and their ISO 639-2 code which can be used with the --language option.

--priority priority

Sets the process priority that mkvmerge(1) runs with. Valid values are 'lowest', 'lower', 'normal', 'higher' and 'highest'. If nothing is given then 'normal' is used. On Unix like systems mkvmerge(1) will use the nice(2) function. Therefore only the super user can use 'higher' and 'highest'. On Windows all values are useable for every user.

Selecting 'lowest' also causes mkvmerge(1) to select idle I/O priority in addition to the lowest possible process priority.

--command-line-charset character-set | Sets the character set to convert strings given on the command line from. It defaults to the character set given by system's current locale. This settings applies to arguments of the following options: --title, --track-name and --attachment-description.
--output-charset character-set | Встановлює вихідний набір символів заданого в командному рядку для конвертації. Типово використовується набір символів згідно поточної локалі системи.
-r, --redirect-output file-name | Writes all messages to the file file-name instead of to the console. While this can be done easily with output redirection there are cases in which this option is needed: when the terminal reinterprets the output before writing it to a file. The character set set with --output-charset is honored.
--flush-on-close | Повідомляє програмі перенести до сховища кешовані в пам’яті дані під час закриття файлів, що були відкриті на запис. Це можна використовувати, щоб запобігти втраті даних при відключенні електроенергії або обійти певні проблеми в операційній системі чи драйверах. Недоліком є те, що мультиплексування займе більше часу, оскільки mkvmerge буде чекати, поки всі дані будуть записані в сховище, перш ніж вийти. Дивіться проблемы 2469 і 2480 баг-трекера MKVToolNix щоб дізнатися про переваги та недоліки.
--ui-language code | Задає примусове використання мовного перекладу code інтерфейсу (наприклад, 'de_DE' для німецького перекладу). Після введення list' як code програма відобразить список доступних перекладів.
--abort-on-warnings | Повідомляє програмі припинити роботу після першого попередження. Код виходу з програми буде 1.

--deterministic seed

Enables the creation of byte-identical files if the same version of mkvmerge(1) is used with the same source files, the same set of options and the same seed. Note that the "date" segment information field is not written in this mode.

The seed can be an arbitrary string and does not have to be a number.

The result of byte-identical files is only guaranteed under the following conditions:

1. The same version of mkvmerge(1) built with the same versions of libEBML and libMatroska is used.

2. The source files used are byte-identical.

3. The same command line options are used in the same order (with the notable exception of --output …).

Using other versions of mkvmerge(1) or other command-line options may result in the same byte-identical file but is not guaranteed to do so.

--debug topic | Увімкнути налагодження для певної функції. Ця опція корисна лише для розробників.
--engage feature | Turn on experimental features. A list of available features can be requested with mkvmerge --engage list. These features are not meant to be used in normal situations.
--gui-mode | Вмикає режим графічного інтерфейсу. У цьому режимі можуть бути виведені спеціально відформатовані рядки, які можуть повідомляти керуючому графічному інтерфейсу, що відбувається. Ці повідомлення мають формат '#GUI#message'. За повідомленням можуть слідувати пари ключ/значення, як у '#GUI#message#key1=value1#key2=value2…'. Ані повідомлення, ані ключі ніколи не перекладаються і завжди виводяться англійською.
@options-file.json | Reads additional command line arguments from the file options-file. See the section about option files for further information.

--capabilities

Lists information about optional features that have been compiled in and exit. The first line output will be the version information. All following lines contain exactly one word whose presence indicates that the feature has been compiled in. These features are:

- 'FLAC' -- reading raw FLAC files and handling FLAC tracks in other containers, e.g. Ogg(tm) or Matroska(tm).

-h, --help | Відображається інформація про використання додатку і відбувається завершення роботи додатку.
-V, --version | Відображається інформація про версію додатку і відбувається завершення роботи додатку.

# 3. Використання

For each file the user can select which tracks mkvmerge(1) should take. They are all put into the file specified with -o. A list of known (and supported) source formats can be obtained with the -l option.

Important:

Важливим є порядок параметрів командного рядка. Будь ласка, прочитайте розділ "Порядок опцій", якщо ви новачок у програмі.

# 4. Option order

The order in which options are entered is important for some options. Options fall into two categories:

1. Options that affect the whole program and are not tied to any input file. These include but are not limited to --command-line-charset, --output or --title. These can appear anywhere on the command line.

2. Options that affect a single input file or a single track in an input file. These options all apply to the following input file on the command line. All options applying to the same input (or to tracks from the same input file) file can be written in any order as long as they all appear before that input file's name. Examples for options applying to an input file are --no-chapters or --chapter-charset. Examples for options applying to a single track are --default-duration or --language.

The options are processed from left to right. If an option appears multiple times within the same scope then the last occurrence will be used. Therefore the title will be set to "Something else" in the following example:

    $ mkvmerge -o output.mkv --title 'This and that' input.avi --title 'Something else'

The following example shows that using the --language option twice is OK because they're used in different scopes. Even though they apply to the same track ID they apply to different input files and therefore have different scopes:

    $ mkvmerge -o output.mkv --language 0:fre français.ogg --language 0:deu deutsch.ogg

# 5. Приклади

Let's assume you have a file called MyMovie.avi and the audio track in a separate file, e.g. 'MyMovie.wav'. First you want to encode the audio to OggVorbis(tm):

    $ oggenc -q4 -oMyMovie.ogg MyMovie.wav

After a couple of minutes you can join video and audio:

    $ mkvmerge -o MyMovie-with-sound.mkv MyMovie.avi MyMovie.ogg

If your AVI already contains an audio track then it will be copied as well (if mkvmerge(1) supports the audio format). To avoid that simply do

    $ mkvmerge -o MyMovie-with-sound.mkv -A MyMovie.avi MyMovie.ogg

After some minutes of consideration you rip another audio track, e.g. the director's comments or another language to 'MyMovie-add-audio.wav'. Encode it again and join it up with the other file:

    $ oggenc -q4 -oMyMovie-add-audio.ogg MyMovie-add-audio.wav
    $ mkvmerge -o MM-complete.mkv MyMovie-with-sound.mkv MyMovie-add-audio.ogg

The same result can be achieved with

    $ mkvmerge -o MM-complete.mkv -A MyMovie.avi MyMovie.ogg MyMovie-add-audio.ogg

Now fire up mplayer(tm) and enjoy. If you have multiple audio tracks (or even video tracks) then you can tell mplayer(tm) which track to play with the '-vid' and '-aid' options. These are 0-based and do not distinguish between video and audio.

If you need an audio track synchronized you can do that easily. First find out which track ID the Vorbis track has with

    $ mkvmerge --identify outofsync.ogg

Тепер ви можете використовувати цей ID у наступному командному рядку:

    $ mkvmerge -o goodsync.mkv -A source.avi -y 12345:200 outofsync.ogg

This would add 200ms of silence at the beginning of the audio track with the ID 12345 taken from 'outofsync.ogg'.

Some movies start synced correctly but slowly drift out of sync. For these kind of movies you can specify a delay factor that is applied to all timestamps -- no data is added or removed. So if you make that factor too big or too small you'll get bad results. An example is that an episode I transcoded was 0.2 seconds out of sync at the end of the movie which was 77340 frames long. At 29.97fps 0.2 seconds correspond to approx. 6 frames. So I did

    $ mkvmerge -o goodsync.mkv -y 23456:0,77346/77340 outofsync.mkv

The result was fine.

The sync options can also be used for subtitles in the same manner.

For text subtitles you can either use some Windows software (like SubRipper(tm)) or the subrip(tm) package found in transcode(1)'s sources in the 'contrib/subrip' directory. The general process is:

1. extract a raw subtitle stream from the source:

       $ tccat -i /path/to/copied/dvd/ -T 1 -L | tcextract -x ps1 -t vob -a 0x20 | subtitle2pgm -o mymovie

2. convert the resulting PGM images to text with gocr:

       $ pgm2txt mymovie

3. spell-check the resulting text files:

       $ ispell -d american *txt

4. convert the text files to a SRT file:

       $ srttool -s -w -i mymovie.srtx -o mymovie.srt

The resulting file can be used as another input file for mkvmerge(1):

    $ mkvmerge -o mymovie.mkv mymovie.avi mymovie.srt

If you want to specify the language for a given track then this is easily done. First find out the ISO 639-2 code for your language. mkvmerge(1) can list all of those codes for you:

    $ mkvmerge --list-languages

Search the list for the languages you need. Let's assume you have put two audio tracks into a Matroska(tm) file and want to set their language codes and that their track IDs are 2 and 3. This can be done with

    $ mkvmerge -o with-lang-codes.mkv --language 2:ger --language 3:dut without-lang-codes.mkv

As you can see you can use the --language switch multiple times.

Maybe you'd also like to have the player use the Dutch language as the default language. You also have extra subtitles, e.g. in English and French, and want to have the player display the French ones by default. This can be done with

    $ mkvmerge -o with-lang-codes.mkv --language 2:ger --language 3:dut --default-track-flag 3 without-lang-codes.mkv --language 0:eng english.srt --default-track-flag 0 --language 0:fre french.srt

If you do not see the language or default track flags that you've specified in mkvinfo(1)'s output then please read the section about default values.

Turn off the compression for an input file.

    $ mkvmerge -o no-compression.mkv --compression -1:none MyMovie.avi --compression -1:none mymovie.srt

# 6. ID доріжок

## 6.1. Regular track IDs

Some of the options for mkvmerge(1) need a track ID to specify which track they should be applied to. Those track IDs are printed by the readers when demuxing the current input file, or if mkvmerge(1) is called with the --identify option. An example for such output:

    $ mkvmerge -i v.mkv
    File 'v.mkv': container: Matroska
    Track ID 0: video (V_MS/VFW/FOURCC, DIV3)
    Track ID 1: audio (A_MPEG/L3)

Do not confuse the track IDs that are assigned to the tracks that are placed in the output MKV file with the track IDs of the input files. Only the input file track IDs are used for options needing these values.

Also note that each input file has its own set of track IDs. Therefore the track IDs for file 'file1.ext' as reported by 'mkvmerge --identify' do not change no matter how many other input files are there or in which position 'file1.ext' is used.

Track IDs are assigned like this:

- AVI files: The video track has the ID 0. The audio tracks get IDs in ascending order starting at 1.

- Файли AAC, AC-3, MP3, SRT і WAV: одна доріжка у цьому файлі отримує ID 0.

- Most other files: The track IDs are assigned in order the tracks are found in the file starting at 0.

The options that use the track IDs are the ones whose description contains 'TID'. The following options use track IDs as well: --audio-tracks, --video-tracks, --subtitle-tracks, --button-tracks and --track-tags.

## 6.2. Special track IDs

There are several IDs that have special meaning and do not occur in the identification output.

The special track ID '-1' is a wild card and applies the given switch to all tracks that are read from an input file.

The special track ID '-2' refers to the chapters in a source file. Currently only the --sync option uses this special ID. As an alternative to --sync -2:… the option --chapter-sync … can be used.

# 7. Текстові файли та перетворення набору символів

Note:

This section applies to all programs in MKVToolNix even if it only mentions mkvmerge(1).

## 7.1. Вступ

All text in a Matroska(tm) file is encoded in UTF-8. This means that mkvmerge(1) has to convert every text file it reads as well as every text given on the command line from one character set into UTF-8. In return this also means that mkvmerge(1)'s output has to be converted back to that character set from UTF-8, e.g. if a non-English translation is used with --ui-language or for text originating from a Matroska(tm) file.

mkvmerge(1) does this conversion automatically based on the presence of a byte order marker (short: BOM) or the system's current locale. How the character set is inferred from the locale depends on the operating system that mkvmerge(1) is run on.

## 7.2. Byte order markers (BOM)

Text files that start with a BOM are already encoded in one representation of UTF. mkvmerge(1) supports the following five modes: UTF-8, UTF-16 Little and Big Endian, UTF-32 Little and Big Endian. Text files with a BOM are automatically converted to UTF-8. Any of the parameters that would otherwise set the character set for such a file (e.g. --sub-charset) is silently ignored.

## 7.3. Linux and Unix-like systems including macOS

On Unix-like systems mkvmerge(1) uses the setlocale(3) system call which in turn uses the environment variables LANG, LC_ALL and LC_CYPE. The resulting character set is often one of UTF-8 or the ISO-8859-* family and is used for all text file operations and for encoding strings on the command line and for output to the console.

## 7.4. Windows

On Windows the default character set used for converting text files is determined by a call to the GetACP() system call.

Reading the command line is done with the GetCommandLineW() function which already returns a Unicode string. Therefore the option --command-line-charset is ignored on Windows.

Output to the console consists of three scenarios:

1. If the output is redirected with the option --redirect-output then the default charset is UTF-8. This can be changed with --output-charset.

2. If the output is redirected with cmd.exe itself, e.g. with mkvinfo file.mkv > info.txt, then the charset is always UTF-8 and cannot be changed.

3. Otherwise (when writing directly to the console) the Windows function WriteConsoleW() is used and the option --output-charset is ignored. The console should be able to output all Unicode characters for which the corresponding language support is installed (e.g. Chinese characters might not be displayed on English Windows versions).

## 7.5. Опції командного рядка

The following options exist that allow specifying the character sets:

- --sub-charset for text subtitle files and for text subtitle tracks stored in container formats for which the character set cannot be determined unambiguously (e.g. Ogg files),

- --chapter-charset for chapter text files and for chapters and file titles stored in container formats for which the character set cannot be determined unambiguously (e.g. Ogg files for chapter information, track and file titles etc; MP4 files for chapter information),

- --command-line-charset for all strings on the command line,

- --output-charset for all strings written to the console or to a file if the output has been redirected with the --redirect-output option. On non-Windows systems the default for the output charset is the system's current charset. On Windows it defaults to UTF-8 both for redirecting with --redirect-output and with cmd.exe itself, e.g. mkvinfo file.mkv > info.txt.

# 8. Файли опцій

An option file is a file mkvmerge(1) can read additional command line arguments from. This can be used in order to circumvent certain limitations of the shell or the operating system when executing external programs like a limited command line length.

An option file contains JSON-formatted data. Its content must be a valid JSON array consisting solely of JSON strings. The file's encoding must be UTF-8. The file should not start with a byte order marker (BOM), but if one exists, it will be skipped.

The rules for escaping special characters inside JSON are the ones in the official JSON specification, RFC 7159.

The option file's name itself must be specified as a command line argument prefixed with a '@' character.

Командний рядок 'mkvextract tracks source.mkv --raw 1:destination.raw' може бути перетворений на наступний конфігураційний файл:

    [
      "-o",
      "c:\\Matroska\\my file.mkv",
      "--title",
      "#65",
      "-A",
      "a movie.avi",
      "sound.ogg"
    ]

The corresponding command would then be 'mkvmerge @options.json'.

# 9. File linking

Matroska(tm) supports file linking which simply says that a specific file is the predecessor or successor of the current file. To be precise, it's not really the files that are linked but the Matroska(tm) segments. As most files will probably only contain one Matroska(tm) segment the following explanations use the term 'file linking' although 'segment linking' would be more appropriate.

Each segment is identified by a unique 128 bit wide segment UID. This UID is automatically generated by mkvmerge(1). The linking is done primarily via putting the segment UIDs (short: SID) of the previous/next file into the segment header information. mkvinfo(1) prints these SIDs if it finds them.

If a file is split into several smaller ones and linking is used then the timestamps will not start at 0 again but will continue where the last file has left off. This way the absolute time is kept even if the previous files are not available (e.g. when streaming). If no linking is used then the timestamps should start at 0 for each file. By default mkvmerge(1) does not use file linking. If you want that you can turn it on with the --link option. This option is only useful if splitting is activated as well.

Regardless of whether splitting is active or not the user can tell mkvmerge(1) to link the produced files to specific SIDs. This is achieved with the options --link-to-previous and --link-to-next. These options accept a segment SID in the format that mkvinfo(1) outputs: 16 hexadecimal numbers between 0x00 and 0xff prefixed with '0x' each, e.g. '0x41 0xda 0x73 0x66 0xd9 0xcf 0xb2 0x1e 0xae 0x78 0xeb 0xb4 0x5e 0xca 0xb3 0x93'. Alternatively a shorter form can be used: 16 hexadecimal numbers between 0x00 and 0xff without the '0x' prefixes and without the spaces, e.g. '41da7366d9cfb21eae78ebb45ecab393'.

If splitting is used then the first file is linked to the SID given with --link-to-previous and the last file is linked to the SID given with --link-to-next. If splitting is not used then the one output file will be linked to both of the two SIDs.

# 10. Значення за замовчуванням

The Matroska(tm) specification states that some elements have a default value. Usually an element is not written to the file if its value is equal to its default value in order to save space. The elements that the user might miss in mkvinfo(1)'s output are the language and the default track flag elements. The default value for the language is English ('eng'), and the default value for the default track flag is true. Therefore if you used --language 0:eng for a track then it will not show up in mkvinfo(1)'s output.

# 11. Вкладення

Maybe you also want to keep some photos along with your Matroska(tm) file, or you're using SSA subtitles and need a special TrueType(tm) font that's really rare. In these cases you can attach those files to the Matroska(tm) file. They will not be just appended to the file but embedded in it. A player can then show those files (the 'photos' case) or use them to render the subtitles (the 'TrueType(tm) fonts' case).

Here's an example how to attach a photo and a TrueType(tm) font to the output file:

    $ mkvmerge -o output.mkv -A video.avi sound.ogg \
      --attachment-description "Me and the band behind the stage in a small get-together" \
      --attachment-mime-type image/jpeg \
      --attach-file me_and_the_band.jpg \
      --attachment-description "The real rare and unbelievably good looking font" \
      --attachment-mime-type application/octet-stream \
      --attach-file really_cool_font.ttf

If a Matroska(tm) containing attachments file is used as an input file then mkvmerge(1) will copy the attachments into the new file. The selection which attachments are copied and which are not can be changed with the options --attachments and --no-attachments.

# 12. Глави

The Matroska(tm) chapter system is more powerful than the old known system used by OGM files. The full specifications can be found at the Matroska website.

mkvmerge(1) supports two kinds of chapter files as its input. The first format, called 'simple chapter format', is the same format that the OGM tools expect. The second format is a XML based chapter format which supports all of Matroska(tm)'s chapter functionality.

Apart from dedicated chapter files mkvmerge(1) can also read chapters from other file formats (e.g. MP4, Ogg, Blu-rays or DVDs).

## 12.1. Простий формат глав

This format consists of pairs of lines that start with 'CHAPTERxx=' and 'CHAPTERxxNAME=' respectively. The first one contains the start timestamp while the second one contains the title. Here's an example:

    CHAPTER01=00:00:00.000
    CHAPTER01NAME=Intro
    CHAPTER02=00:02:30.000
    CHAPTER02NAME=Baby prepares to rock
    CHAPTER03=00:02:42.300
    CHAPTER03NAME=Baby rocks the house

mkvmerge(1) will transform every pair or lines into one Matroska(tm) ChapterAtom. It does not set any ChapterTrackNumber which means that the chapters all apply to all tracks in the file.

As this is a text file character set conversion may need to be done. See the section about text files and character sets for an explanation how mkvmerge(1) converts between character sets.

## 12.2. Формат глав, що базується на XML

Формат глав, що базується на XML, виглядає як у наступному прикладі:

    <?xml version="1.0" encoding="ISO-8859-1"?>
    <!DOCTYPE Chapters SYSTEM "matroskachapters.dtd">
    <Chapters>
      <EditionEntry>
        <ChapterAtom>
          <ChapterTimeStart>00:00:30.000</ChapterTimeStart>
          <ChapterTimeEnd>00:01:20.000</ChapterTimeEnd>
          <ChapterDisplay>
            <ChapterString>A short chapter</ChapterString>
            <ChapterLanguage>eng</ChapterLanguage>
          </ChapterDisplay>
          <ChapterAtom>
            <ChapterTimeStart>00:00:46.000</ChapterTimeStart>
            <ChapterTimeEnd>00:01:10.000</ChapterTimeEnd>
            <ChapterDisplay>
              <ChapterString>A part of that short chapter</ChapterString>
              <ChapterLanguage>eng</ChapterLanguage>
            </ChapterDisplay>
          </ChapterAtom>
        </ChapterAtom>
      </EditionEntry>
    </Chapters>

With this format three things are possible that are not possible with the simple chapter format:

1. The timestamp for the end of the chapter can be set,

2. chapters can be nested,

3. the language and country can be set.

The mkvtoolnix distribution contains some sample files in the doc subdirectory which can be used as a basis.

The following lists the supported XML tags, their data types and, where appropriate, the valid range for their values:

    Chapters (master)
      EditionEntry (master)
        EditionUID (unsigned integer, valid range: 1 <= value)
        EditionFlagHidden (unsigned integer, valid range: 0 <= value <= 1)
        EditionFlagDefault (unsigned integer, valid range: 0 <= value <= 1)
        EditionFlagOrdered (unsigned integer, valid range: 0 <= value <= 1)
        ChapterAtom (master)
          ChapterAtom (master)
          ChapterUID (unsigned integer, valid range: 1 <= value)
          ChapterTimeStart (unsigned integer)
          ChapterTimeEnd (unsigned integer)
          ChapterFlagHidden (unsigned integer, valid range: 0 <= value <= 1)
          ChapterFlagEnabled (unsigned integer, valid range: 0 <= value <= 1)
          ChapterSegmentUID (binary, valid range: 1 <= length in bytes)
          ChapterSegmentEditionUID (unsigned integer, valid range: 1 <= value)
          ChapterPhysicalEquiv (unsigned integer)
          ChapterTrack (master)
            ChapterTrackNumber (unsigned integer, valid range: 1 <= value)
          ChapterDisplay (master)
            ChapterString (UTF-8 string)
            ChapterLanguage (UTF-8 string)
            ChapterCountry (UTF-8 string)
          ChapterProcess (master)
            ChapterProcessCodecID (unsigned integer)
            ChapterProcessPrivate (binary)
            ChapterProcessCommand (master)
              ChapterProcessTime (unsigned integer)
              ChapterProcessData (binary)

## 12.3. Reading chapters from Blu-rays

mkvmerge(1) can read chapters from unencrypted Blu-rays. For that you can use the path to one of the MPLS play lists with the --chapters parameter.

Example: --chapters /srv/blurays/BigBuckBunny/BDMV/PLAYLIST/00001.mpls

## 12.4. Reading chapters from DVDs

When MKVToolNix is compiled with the libdvdread(tm) library, mkvmerge(1) can read chapters from DVDs. For that you can use the path to one of the folders or files on the DVD with the --chapters parameter. As DVDs can contain more than one title and each title has its own set of chapters, you can append a colon and the desired title number to the end of the file name argument. The title number defaults to 1.

Приклад: --generate-chapters interval:45s

## 12.5. Загальні примітки

When splitting files mkvmerge(1) will correctly adjust the chapters as well. This means that each file only includes the chapter entries that apply to it, and that the timestamps will be offset to match the new timestamps of each output file.

mkvmerge(1) is able to copy chapters from Matroska(tm) source files unless this is explicitly disabled with the --no-chapters option. The chapters from all sources (Matroska(tm) files, Ogg files, MP4 files, chapter text files) are usually not merged but end up in separate ChapterEditions. Only if chapters are read from several Matroska(tm) or XML files that share the same edition UIDs will chapters be merged into a single ChapterEdition. If such a merge is desired in other situations as well then the user has to extract the chapters from all sources with mkvextract(1) first, merge the XML files manually and mux them afterwards.

# 13. Теги

## 13.1. Вступ

Matroska(tm)'s tag system is similar to that of other containers: a set of KEY=VALUE pairs. However, in Matroska(tm) these tags can also be nested, and both the KEY and the VALUE are elements of their own. The example file example-tags-2.xml shows how to use this system.

## 13.2. Scope of the tags

Matroska(tm) tags do not automatically apply to the complete file. They can, but they also may apply to different parts of the file: to one or more tracks, to one or more chapters, or even to a combination of both. The Matroska specification gives more details about this fact.

One important fact is that tags are linked to tracks or chapters with the Targets Matroska(tm) tag element, and that the UIDs used for this linking are not the track IDs mkvmerge(1) uses everywhere. Instead the numbers used are the UIDs which mkvmerge(1) calculates automatically (if the track is taken from a file format other than Matroska(tm)) or which are copied from the source file if the track's source file is a Matroska(tm) file. Therefore it is difficult to know which UIDs to use in the tag file before the file is handed over to mkvmerge(1).

mkvmerge(1) knows two options with which you can add tags to Matroska(tm) files: The --global-tags and the --tags options. The difference is that the former option, --global-tags, will make the tags apply to the complete file by removing any of those Targets elements mentioned above. The latter option, --tags, automatically inserts the UID that mkvmerge(1) generates for the tag specified with the TID part of the --tags option.

## 13.3. Приклад

повідомляє

    $ mkvmerge -o file.mkv --tags 0:tags.xml file.avi

## 13.4. Tag file format

mkvmerge(1) supports a XML based tag file format. The format is very closely modeled after the Matroska specification. Both the binary and the source distributions of MKVToolNix come with a sample file called example-tags-2.xml which simply lists all known tags and which can be used as a basis for real life tag files.

The basics are:

- The outermost element must be <Tags>.

- One logical tag is contained inside one pair of <Tag> XML tags.

- White spaces directly before and after tag contents are ignored.

## 13.5. Типи даних

The new Matroska(tm) tagging system only knows two data types, a UTF-8 string and a binary type. The first is used for the tag's name and the <String> element while the binary type is used for the <Binary> element.

As binary data itself would not fit into a XML file mkvmerge(1) supports two other methods of storing binary data. If the contents of a XML tag starts with '@' then the following text is treated as a file name. The corresponding file's content is copied into the Matroska(tm) element.

Otherwise the data is expected to be Base64 encoded. This is an encoding that transforms binary data into a limited set of ASCII characters and is used e.g. in email programs. mkvextract(1) will output Base64 encoded data for binary elements.

The deprecated tagging system knows some more data types which can be found in the official Matroska(tm) tag specs. As mkvmerge(1) does not support this system anymore these types aren't described here.

## 13.6. Known tags for the XML file format

The following lists the supported XML tags, their data types and, where appropriate, the valid range for their values:

    Tags (master)
      Tag (master)
        Targets (master)
          TargetTypeValue (unsigned integer)
          TargetType (UTF-8 string)
          TrackUID (unsigned integer)
          EditionUID (unsigned integer)
          ChapterUID (unsigned integer)
          AttachmentUID (unsigned integer)
        Simple (master)
          Simple (master)
          Name (UTF-8 string)
          TagLanguage (UTF-8 string)
          DefaultLanguage (unsigned integer)
          String (UTF-8 string)
          Binary (binary)

# 14. The segment info XML files

With a segment info XML file it is possible to set certain values in the "segment information" header field of a Matroska(tm) file. All of these values cannot be set via other command line options.

Other "segment information" header fields can be set via command line options but not via the XML file. This includes e.g. the --title and the --timestamp-scale options.

There are other elements that can be set neither via command line options nor via the XML files. These include the following elements: DateUTC (also known as the "muxing date"), MuxingApp, WritingApp and Duration. They're always set by mkvmerge(1) itself.

The following lists the supported XML tags, their data types and, where appropriate, the valid range for their values:

    Info (master)
      SegmentUID (binary, valid range: length in bytes == 16)
      SegmentFilename (UTF-8 string)
      PreviousSegmentUID (binary, valid range: length in bytes == 16)
      PreviousSegmentFilename (UTF-8 string)
      NextSegmentUID (binary, valid range: length in bytes == 16)
      NextSegmentFilename (UTF-8 string)
      SegmentFamily (binary, valid range: length in bytes == 16)
      ChapterTranslate (master)
        ChapterTranslateEditionUID (unsigned integer)
        ChapterTranslateCodec (unsigned integer)
        ChapterTranslateID (binary)

# 15. Matroska file layout

The Matroska(tm) file layout is quite flexible. mkvmerge(1) will render a file in a predefined way. The resulting file looks like this:

[EBML head] [segment {meta seek #1} [segment information] [track information] {attachments} {chapters} [cluster 1] {cluster 2} ... {cluster n} {cues} {meta seek #2} {tags}]

The elements in curly braces are optional and depend on the contents and options used. A couple of notes:

- meta seek #1 includes only a small number of level 1 elements, and only if they actually exist: attachments, chapters, cues, tags, meta seek #2. Older versions of mkvmerge(1) used to put the clusters into this meta seek element as well. Therefore some imprecise guessing was necessary to reserve enough space. It often failed. Now only the clusters are stored in meta seek #2, and meta seek #1 refers to the meta seek element #2.

- Attachment, chapter and tag elements are only present if they were added.

The shortest possible Matroska(tm) file would look like this:

[EBML head] [segment [segment information] [track information] [cluster 1]]

This might be the case for audio-only files.

# 16. External timestamp files

mkvmerge(1) allows the user to chose the timestamps for a specific track himself. This can be used in order to create files with variable frame rate video or include gaps in audio. A frame in this case is the unit that mkvmerge(1) creates separately per Matroska(tm) block. For video this is exactly one frame, for audio this is one packet of the specific audio type. E.g. for AC-3 this would be a packet containing 1536 samples.

Timestamp files that are used when tracks are appended to each other must only be specified for the first part in a chain of tracks. For example if you append two files, v1.avi and v2.avi, and want to use timestamps then your command line must look something like this:

    $ mkvmerge ... --timestamps 0:my_timestamps.txt v1.avi +v2.avi

There are four formats that are recognized by mkvmerge(1). The first line always contains the version number. Empty lines, lines containing only whitespace and lines beginning with '#' are ignored.

## 16.1. Timestamp file format v1

This format starts with the version line. The second line declares the default number of frames per second. All following lines contain three numbers separated by commas: the start frame (0 is the first frame), the end frame and the number of frames in this range. The FPS is a floating point number with the dot '.' as the decimal point. The ranges can contain gaps for which the default FPS is used. An example:

    # timestamp format v1
    assume 27.930
    800,1000,25
    1500,1700,30

## 16.2. Timestamp file format v2

In this format each line contains a timestamp for the corresponding frame. This timestamp must be given in millisecond precision. It can be a floating point number, but it doesn't have to be. You have to give at least as many timestamp lines as there are frames in the track. The timestamps in this file must be sorted. Example for 25fps:

    # timestamp format v2
    0
    40
    80

## 16.3. Timestamp file format v3

In this format each line contains a duration in seconds followed by an optional number of frames per second. Both can be floating point numbers. If the number of frames per second is not present the default one is used. For audio you should let the codec calculate the frame timestamps itself. For that you should be using 0.0 as the number of frames per second. You can also create gaps in the stream by using the 'gap' keyword followed by the duration of the gap. Example for an audio file:

    # timestamp format v3
    assume 0.0
    25.325
    7.530,38.236
    gap, 10.050
    2.000,38.236

## 16.4. Timestamp file format v4

This format is identical to the v2 format. The only difference is that the timestamps do not have to be sorted. This format should almost never be used.

# 17. Коди завершення

mkvmerge(1) exits with one of three exit codes:

- 0 -- This exit code means that muxing has completed successfully.

- 1 -- In this case mkvmerge(1) has output at least one warning, but muxing did continue. A warning is prefixed with the text 'Warning:'. Depending on the issues involved the resulting file might be ok or not. The user is urged to check both the warning and the resulting file.

- 2 -- This exit code is used after an error occurred. mkvmerge(1) aborts right after outputting the error message. Error messages range from wrong command line arguments over read/write errors to broken files.

# 18. Змінні середовища

mkvmerge(1) uses the default variables that determine the system's locale (e.g. LANG and the LC_* family). Additional variables:

Option | Description
--- | ---
MKVMERGE_DEBUG, MKVTOOLNIX_DEBUG і їх коротка форма MTX_DEBUG | The content is treated as if it had been passed via the --debug option.
MKVMERGE_ENGAGE, MKVTOOLNIX_ENGAGE і їх коротка форма MTX_ENGAGE | The content is treated as if it had been passed via the --engage option.

# 19. Дивіться також

mkvmerge(1), mkvinfo(1), mkvpropedit(1), mkvtoolnix-gui(1)

# 20. WWW

Остання версія завжди може бути знайдена на веб-сторінці MKVToolNix.